---
title: Plugin: PixArt RF
---

## Introduction

This plugin allows the user to update any supported Pixart RF Device using a
custom HID-based OTA protocol

## Firmware Format

The daemon will decompress the cabinet archive and extract a firmware blob in
an unspecified binary file format.

This plugin supports the following protocol ID:

* `com.pixart.rf`

## GUID Generation

These devices use the standard HIDRAW DeviceInstanceId values for both
Pixart Imaging, Inc and Primax Electronics, Ltd, e.g.

* `HIDRAW\VEN_093A&DEV_2801`
* `HIDRAW\VEN_0461&DEV_4EEF`
* `HIDRAW\VEN_0461&DEV_4EEF&NAME_${NAME}`
* `HIDRAW\VEN_0461&DEV_4EEF&MODEL_${MODEL_NAME}`

Additionally, a custom GUID values including the name is used, e.g.

## Update Behavior

The firmware is deployed when the device is in normal runtime mode, and the
device will reset when the new firmware has been written.

## Quirk Use

This plugin uses the following plugin-specific quirks:

### `Flags=is-hpac`

Use HPAC firmware header.

## Vendor ID Security

The vendor ID is set from the USB vendor, in this instance set to `USB:0x093A`

## External Interface Access

This plugin requires ioctl `HIDIOCSFEATURE` and `HIDIOCGFEATURE` access.

## Version Considerations

This plugin has been available since fwupd version `1.5.5`.
