# libfwupdplugin

This library is only partially API and ABI stable. Keeping unused, unsafe and
deprecated functions around forever is a maintenance burden and so symbols are
removed when branching for new minor versions.

Use `./contrib/migrate.py` to migrate up out-of-tree plugins to the new API.

> [!IMPORTANT]
> Plugins should be upstream!

## 1.5.5

* `fu_common_is_cpu_intel()`: Use `fu_common_get_cpu_vendor()` instead.
* `fu_firmware_strparse_uintXX()`: Use `fu_firmware_strparse_uintXX_safe()` instead.
* `fu_plugin_get_usb_context()`: Remove, as no longer required.
* `fu_plugin_set_usb_context()`: Remove, as no longer required.
* `fu_plugin_runner_usb_device_added()`: Use `fu_plugin_runner_backend_device_added()` instead.
* `fu_plugin_runner_udev_device_added()`: Use `fu_plugin_runner_backend_device_added()` instead.
* `fu_plugin_runner_udev_device_changed()`: Use `fu_plugin_runner_backend_device_added()` instead.
* `FuHidDevice->open()`: Use the `FuDevice` superclass instead.
* `FuHidDevice->close()`: Use the `FuDevice` superclass instead.
* `FuUsbDevice->probe()`: Use the `FuDevice` superclass instead.
* `FuUsbDevice->open()`: Use the `FuDevice` superclass instead.
* `FuUsbDevice->close()`: Use the `FuDevice` superclass instead.
* `FuUdevDevice->to_string()`: Use the `FuDevice` superclass instead.
* `FuUdevDevice->probe()`: Use the `FuDevice` superclass instead.
* `FuUdevDevice->open()`: Use the `FuDevice` superclass instead.
* `FuUdevDevice->close()`: Use the `FuDevice` superclass instead.

## 1.5.6

* `fu_device_get_protocol()`: Use `fu_device_get_protocols()` instead.
* `fu_device_set_protocol()`: Use `fu_device_add_protocol()` instead.

## 1.6.2

* `fu_device_has_custom_flag()`: Use `fu_device_has_private_flag()` instead.

## 1.6.3

* `fu_device_sleep_with_progress()`: Use `fu_progress_sleep()` instead -- but be aware the unit of time has changed from *seconds* to *milliseconds*.
* `fu_device_get_status()`: Use `fu_progress_get_status()` instead.
* `fu_device_set_status()`: Use `fu_progress_set_status()` instead.
* `fu_device_get_progress()`: Use `fu_progress_get_percentage()` instead.
* `fu_device_set_progress_full()`: Use `fu_progress_set_percentage_full()` instead.
* `fu_device_set_progress()`: Use `fu_progress_set_steps()`, `fu_progress_add_step()` and `fu_progress_done()` -- see the `FuProgress` docs for more details!

## 1.8.2

* `fu_udev_device_pread_full()`: Use `fu_udev_device_pread()` instead -- as the latter now specifies the buffer length.
* `fu_udev_device_pread_full()`: Use `fu_udev_device_pwrite()` instead -- as the latter now specifies the buffer length.
* `fu_udev_device_ioctl_full()`: Use `fu_udev_device_ioctl()` instead -- as the latter now always specifies the timeout.
* `fu_udev_device_new_full()`: Use `fu_udev_device_new()` instead -- as the latter always specifies the context.
* `fu_usb_device_new_full()`: Use `fu_usb_device_new()` instead -- as the latter always specifies the context.
* `fu_device_new_with_context()`: Use `fu_device_new()` instead -- as the latter always specifies the context.
* `fu_plugin_has_custom_flag()`: Use `fu_plugin_has_private_flag()` instead.
* `fu_efivar_secure_boot_enabled_full()`: Use `fu_efivars_get_secure_boot()` instead -- as the latter always specifies the error.
* `fu_progress_add_step()`: Add a 4th parameter to the function to specify the nice name for the step, or NULL.
* `fu_backend_setup()`: Now requires a `FuProgress`, although it can be ignored.
* `fu_backend_coldplug`: Now requires a `FuProgress`, although it can be ignored.
* `FuPluginVfuncs->setup`: Now requires a `FuProgress`, although it can be ignored.
* `FuPluginVfuncs->coldplug`: Now requires a `FuProgress`, although it can be ignored.
* `fu_common_crc*`: Use `fu_crc` prefix, i.e. remove the `_common`
* `fu_common_sum*`: Use `fu_sum` prefix, i.e. remove the `_common`
* `fu_byte_array_set_size_full()`: Use `fu_byte_array_set_size` instead -- as the latter now always specifies the fill char.
* `fu_common_string*`: Use `fu_string` prefix, i.e. remove the `_common`
* `fu_common_bytes*`: Use `fu_bytes` prefix, i.e. remove the `_common`
* `fu_common_set_contents_bytes()`: Use `fu_bytes_set_contents()` instead
* `fu_common_get_contents_bytes()`: Use `fu_bytes_get_contents()` instead
* `fu_common_read*`: Use `fu_memread` prefix, i.e. replace the `_common` with `_mem`
* `fu_common_write*`: Use `fu_memwrite` prefix, i.e. replace the `_common` with `_mem`
* `fu_common_bytes_compare_raw()`: Use `fu_memcmp_safe()` instead
* `fu_common_spawn_sync()`: Use `g_spawn_sync()` instead, or ideally not at all!
* `fu_common_extract_archive()`: Use `FuZipFirmware()` instead.
* `fu_common_instance_id_strsafe()`: Use `fu_device_add_instance_strsafe()` instead.
* `fu_common_kernel_locked_down()`: Use `fu_kernel_locked_down` instead.
* `fu_common_check_kernel_version()`: Use `fu_kernel_check_version` instead.
* `fu_common_get_firmware_search_path()`: Use `fu_kernel_get_firmware_search_path` instead.
* `fu_common_set_firmware_search_path()`: Use `fu_kernel_set_firmware_search_path` instead.
* `fu_common_reset_firmware_search_path()`: Use `fu_kernel_reset_firmware_search_path` instead.
* `fu_common_firmware_builder()`: You should not be using this.
* `fu_common_realpath()`: You should not be using this.
* `fu_common_uri_get_scheme()`: You should not be using this.
* `fu_common_dump*`: Use `fu_dump` prefix, i.e. remove the `_common`
* `fu_common_error_array_get_best()`: You should not be using this.
* `fu_common_cpuid()`: Use `fu_cpuid` instead.
* `fu_common_get_cpu_vendor()`: Use `fu_cpu_get_vendor` instead.
* `fu_common_vercmp_full()`: Use `fu_version_compare()` instead.
* `fu_version_ensure_semver()`: Use `fu_version_ensure_semver()` instead.
* `fu_common_version_from_uint*()`: Use `fu_version_from_uint*()` instead.
* `fu_common_strtoull()`: Use `fu_strtoull()` instead -- as the latter always specifies the error.
* `fu_smbios_to_string()`: Use `fu_firmware_to_string()` instead -- as `FuSmbios` is a `FuFirmware` superclass.
* `fu_common_cab_build_silo()`: You should not be using this.
* `fu_i2c_device_read_full()`: Use `fu_i2c_device_read` instead.
* `fu_i2c_device_write_full()`: Use `fu_i2c_device_write` instead.
* `fu_firmware_parse_bytes()`: Remove the `addr_end` parameter, and ensure that `offset` is a `gsize`.

## 1.8.5

* `fu_volume_new_esp_default()`: Use `fu_context_get_esp_volumes()` instead.
* `fu_plugin_set_secure_config_value()`: Set `FWUPD_PLUGIN_FLAG_SECURE_CONFIG` and use `fu_plugin_set_config_value()`

## 1.8.7

* `fu_mei_device_connect()`: Drop the explicit GUID parameter and match in the quirk file instead.
* `fu_context_get_smbios_data()`: Add a `GError`

## 1.9.1

* `fu_plugin_get_config_value()`: Add the default value as the last parameter
* `fu_plugin_get_config_value_boolean()`: Add the default value as the last parameter

## 1.9.6

* `fu_security_attrs_get_by_appstream_id()`: Add a `GError`

## 1.9.8

* `fu_device_build_instance_id_quirk": rename to`fu_device_build_instance_id_full()`
* `fu_smbios_get_data()`: Now returns a array of `GByte`s
* `fu_udev_device_get_fd()`: Use `fu_udev_device_get_io_channel()` instead
* `fu_device_emit_request()`: Add `FuProgress` and `GError`
* `fu_device_set_version_from_uint16()`: Use `fu_version_from_uint16()` from `FuDeviceClass->convert_version` instead
* `fu_device_set_version_from_uint24()`: Use `fu_version_from_uint24()` from `FuDeviceClass->convert_version` instead
* `fu_device_set_version_from_uint32()`: Use `fu_version_from_uint32()` from `FuDeviceClass->convert_version` instead
* `fu_device_set_version_from_uint64()`: Use `fu_version_from_uint64()` from `FuDeviceClass->convert_version` instead

## 2.0.0

* `fu_hid_device_parse_descriptor()`: Use `fu_hid_device_parse_descriptors()` instead
* `fu_io_channel_new_file()`: Add some `FuIoChannelOpenFlags`, e.g. `FU_IO_CHANNEL_OPEN_FLAG_READ|FU_IO_CHANNEL_OPEN_FLAG_WRITE`
* `fu_udev_device_set_flags()`: Use `fu_udev_device_add_flag()` instead
* `fu_udev_device_get_slot_depth()`: Use `fu_udev_device_get_subsystem_depth()` instead
* `fu_usb_device_is_open()`: Use `fu_device_has_private_flag(device, FU_DEVICE_PRIVATE_FLAG_IS_OPEN)` instead
* `fu_udev_device_ioctl`: Add some `FuIoctlFlags`, e.g. `FU_IOCTL_FLAG_RETRY`
* `fu_udev_device_write_sysfs()`: Add a timeout in milliseconds
* `fu_udev_device_get_sysfs_attr_uint64()`: Use `fu_udev_device_read_sysfs()` instead
* `fu_udev_device_get_sysfs_attr`: Use `fu_udev_device_read_sysfs()` instead
* `fu_i2c_device_get_bus_number()`: Use `fu_udev_device_get_number()` instead
* `fu_usb_device_set_open_retry_count()`: Use `FU_DEVICE_PRIVATE_FLAG_RETRY_OPEN` instead
* `FWUPD_DEVICE_FLAG_INSTALL_PARENT_FIRST`: Use `FU_DEVICE_PRIVATE_FLAG_INSTALL_PARENT_FIRST` instead
* `FWUPD_DEVICE_FLAG_REGISTERED`: Use `FU_DEVICE_PRIVATE_FLAG_REGISTERED` instead
* `FWUPD_DEVICE_FLAG_ADD_COUNTERPART_GUIDS`: Use `FU_DEVICE_PRIVATE_FLAG_ADD_COUNTERPART_GUIDS` instead
* `FWUPD_DEVICE_FLAG_USE_RUNTIME_VERSION`: Use `FU_DEVICE_PRIVATE_FLAG_USE_RUNTIME_VERSION` instead
* `FWUPD_DEVICE_FLAG_SKIPS_RESTART`: Use `FU_DEVICE_PRIVATE_FLAG_SKIPS_RESTART` instead
* `FU_UDEV_DEVICE_FLAG_VENDOR_FROM_PARENT`: Use `fu_device_get_backend_parent_with_subsystem()` and copy properties instead
* `fu_udev_device_is_pci_base_cls`: Put logic in `FuPciDevice` if needed, but consider what you are doing
* `fu_udev_device_get_cls`: Put logic in `FuPciDevice` if needed, or use a quirk instead
* `fu_udev_device_get_vendor`: Use `fu_device_get_vid()` instead
* `fu_udev_device_set_vendor`: Use `fu_device_set_vid()` instead
* `fu_udev_device_get_model`: Use `fu_device_get_pid()` instead
* `fu_udev_device_set_model`: Use `fu_device_set_pid()` instead
* `fu_udev_device_get_subsystem_vendor`: Use `fu_pci_device_get_subsystem_vid()` instead
* `fu_udev_device_get_subsystem_model`: Use `fu_pci_device_get_subsystem_pid()` instead
* `fu_udev_device_get_revision`: Use `fu_pci_device_get_revision()` instead
* `fu_udev_device_set_revision`: Use `fu_pci_device_set_revision()` instead
* `fu_firmware_parse_full()`: Use `fu_firmware_parse_bytes()` instead
* `fu_firmware_parse()`: Use `fu_firmware_parse_bytes()` by adding an offset of 0x0

## 2.0.2

* `fu_chunk_array_new_from_bytes()`: Add a page size, typically `FU_CHUNK_PAGESZ_NONE`
* `fu_chunk_array_new_from_stream()`: Add a page size, typically `FU_CHUNK_PAGESZ_NONE`
* `fu_udev_device_ioctl()`: Use `fu_udev_device_ioctl_new()` instead
* `FuUdevDeviceIoctlFlags`: Use `FuIoctlFlags` instead

## 2.0.6

* `fu_kernel_get_firmware_search_path()`: Use `FuKernelSearchPathLocker` instead.
* `fu_kernel_set_firmware_search_path()`: Use `FuKernelSearchPathLocker` instead.
* `fu_kernel_reset_firmware_search_path()`: Use `FuKernelSearchPathLocker` instead.

## 2.0.7

* `fu_device_write_firmware()`: Use `FuFirmware` rather than a `GInputStream`.
* `fu_bytes_pad()`: Add a data byte, typically `0xFF`.
* `fu_smbios_get_string()`: Add an expected structure length, typically `FU_SMBIOS_STRUCTURE_LENGTH_ANY`.
* `fu_smbios_get_integer()`: Add an expected structure length, typically `FU_SMBIOS_STRUCTURE_LENGTH_ANY`.
* `fu_smbios_get_data()`: Add an expected structure length, typically `FU_SMBIOS_STRUCTURE_LENGTH_ANY`.
* `fu_context_get_smbios_string()`: Add an expected structure length, typically `FU_SMBIOS_STRUCTURE_LENGTH_ANY`.
* `fu_context_get_smbios_integer()`: Add an expected structure length, typically `FU_SMBIOS_STRUCTURE_LENGTH_ANY`.
* `fu_context_get_smbios_data()`: Add an expected structure length, typically `FU_SMBIOS_STRUCTURE_LENGTH_ANY`.

## 2.0.11

* `fu_device_read_firmware()`: Add `FuFirmwareParseFlags` to `fu_device_read_firmware`.

## 2.0.12

* Plugins that don't allow devices to function 100% through probe should use `FWUPD_PLUGIN_FLAG_MUTABLE_ENUMERATION`
* `fu_device_get_contents_bytes()`: Add a maximum read size, typically `G_MAXSIZE`

## 2.0.14

* `fu_error_convert()`: Use `fwupd_error_convert()` instead

## 2.0.17

* `fu_firmware_add_image_full()`: Use `fu_firmware_add_image()` instead.
* `fu_firmware_add_image()`: Add a `GError` and check the return value.

## 2.0.18

* `fu_input_stream_find()`: Add a start offset, typically `0x0`.
* `fu_device_get_parent()`: Add a `GError`
* `fu_device_get_proxy()`: Add a `GError`

## 2.1.1

* `fu_cab_firmware_set_only_basename()`: Use `FU_FIRMWARE_PARSE_FLAG_ONLY_BASENAME` instead.
* `fu_context_add_firmware_gtype()`: Drop the `id` parameter.
* `fu_firmware_build_from_xml()`: Use `fu_firmware_new_from_xml()` instead.
* `fu_firmware_build_from_filename()`: Use `fu_firmware_new_from_filename()` instead.
* `FuArchive`: Use `FuZipFirmware` or `FuCabArchive` instead.
* `FuArchiveFirmware`: Use `FuZipFirmware` instead.
* `fu_path_from_kind()`: Use `fu_path_store_get_path()` of `fu_context_get_path()` instead.
* `fu_path_build()`: Use `fu_path_store_build_filename()` or `fu_context_build_filename()` instead.
* `fu_plugin_device_add()`: Use `fu_plugin_add_device()` instead.
* `fu_plugin_device_remove()`: Use `fu_plugin_remove_device()` instead.
* `fu_cfi_device_new()`: Use a proxy rather than a context.

## 2.1.2

* `fu_unix_seekable_input_stream_new()`: Add `GError`
* `fu_chunk_array_new()`: Add `GError`
* `fu_chunk_array_mutable_new()`: Add `GError`
* `fu_composite_input_stream_add_bytes()`: Add `GError`
* `fu_composite_input_stream_add_partial_stream()`: Add `GError`
* `fu_progress_get_percentage()`: Convert `guint` to `gdouble`
* `fu_progress_set_percentage()`: Convert `guint` to `gdouble`
